#!/usr/bin/env bash

# The battery, for the shell and the Power page.
#
#   panama-battery paths            resolve which sysfs files to watch
#   panama-battery status           one JSON reading, for scripts and contracts
#   panama-battery set-threshold N  cap charging at N% (needs root)
#
# `paths` exists so the shell does not have to poll a subprocess. Globbing is
# the one thing QML cannot do -- a battery is BAT0 on most machines, BAT1 on
# some, CMB0 on a few, and the mains supply is AC, AC0, ADP1 or ACAD depending
# on the firmware -- so this resolves the names once and the shell reads the
# files directly from then on, the way Vitals.qml reads procfs.
#
# Which machine has what is panama-hw's question, so the search lives there and
# this asks it rather than keeping a second copy of the answer.
#
# Charge thresholds are a root write to a sysfs attribute, and the only part of
# this that needs privilege. It goes through panama-sudo so the prompt names
# what is being changed, rather than asking for a password with polkit's
# generic "run a program as another user".

set -uo pipefail

PANAMA_PATH="${PANAMA_PATH:-$HOME/.local/share/Panama}"
HW="$PANAMA_PATH/bin/panama-hw"
SYS="${PANAMA_HW_SYS:-/sys}"

battery_dir() {
    [[ -x "$HW" ]] || return 1
    "$HW" battery-path 2>/dev/null
}

# Every system battery, for the machines that have two. The primary pack
# answers `paths` and drives the watch files; these answer the questions
# where ignoring the second pack gives a wrong answer -- the total charge,
# and which packs a threshold write must reach.
all_battery_dirs() {
    local supply type scope
    for supply in "$SYS"/class/power_supply/*; do
        [[ -r "$supply/type" ]] || continue
        type="$(cat "$supply/type" 2>/dev/null)"
        [[ "$type" == "Battery" ]] || continue
        scope="$(cat "$supply/scope" 2>/dev/null || echo System)"
        [[ "$scope" == "Device" ]] && continue
        printf '%s\n' "$supply"
    done
}

# The mains supply, if the machine has one. A desktop has none, and that is
# not an error: panama-hw's `ac` predicate treats "no mains at all" as being on
# wall power, and the shell falls back to the same assumption.
mains_dir() {
    local supply
    for supply in "$SYS"/class/power_supply/*; do
        [[ -r "$supply/type" ]] || continue
        [[ "$(cat "$supply/type" 2>/dev/null)" == "Mains" ]] || continue
        printf '%s\n' "$supply"
        return 0
    done
    return 1
}

read_int() {
    local file="$1" value
    [[ -r "$file" ]] || return 1
    value="$(cat "$file" 2>/dev/null)" || return 1
    [[ "$value" =~ ^[0-9]+$ ]] || return 1
    printf '%s\n' "$value"
}

cmd_paths() {
    local battery mains threshold=""
    battery="$(battery_dir)" || battery=""
    mains="$(mains_dir)" || mains=""

    # Only report the threshold file when it exists AND is writable through
    # root -- a machine whose kernel exposes a read-only stub would otherwise
    # get a control that silently does nothing.
    if [[ -n "$battery" && -r "$battery/charge_control_end_threshold" ]]; then
        threshold="$battery/charge_control_end_threshold"
    fi

    printf '{"battery":"%s","mains":"%s","threshold":"%s"}\n' \
        "$battery" "$mains" "$threshold"
}

cmd_status() {
    local battery mains capacity="" state="Unknown" online=1 threshold=0
    battery="$(battery_dir)" || battery=""
    mains="$(mains_dir)" || mains=""

    if [[ -n "$battery" ]]; then
        capacity="$(read_int "$battery/capacity")" || capacity=""
        [[ -r "$battery/status" ]] && state="$(cat "$battery/status" 2>/dev/null)"
        threshold="$(read_int "$battery/charge_control_end_threshold")" || threshold=0

        # With two packs, one pack's percentage is not the machine's: sum the
        # stored and full energy across every system battery and answer with
        # the real total. Single-battery machines never reach this.
        local dirs=() dir now full total_now=0 total_full=0
        mapfile -t dirs < <(all_battery_dirs)
        if (( ${#dirs[@]} > 1 )); then
            for dir in "${dirs[@]}"; do
                now="$(read_int "$dir/energy_now" || read_int "$dir/charge_now")" || continue
                full="$(read_int "$dir/energy_full" || read_int "$dir/charge_full")" || continue
                total_now=$(( total_now + now ))
                total_full=$(( total_full + full ))
            done
            (( total_full > 0 )) && capacity=$(( (total_now * 100 + total_full / 2) / total_full ))
        fi
    fi
    if [[ -n "$mains" ]]; then
        online="$(read_int "$mains/online")" || online=0
    fi

    printf '{"available":%s,"percent":%s,"status":"%s","acOnline":%s,"chargeLimit":%s}\n' \
        "$([[ -n "$capacity" ]] && echo true || echo false)" \
        "${capacity:-0}" "$state" \
        "$([[ "$online" == "1" ]] && echo true || echo false)" \
        "$threshold"
}

cmd_set_threshold() {
    local value="${1:-}" battery file
    [[ "$value" =~ ^[0-9]+$ ]] || { echo 'set-threshold needs a percentage' >&2; return 2; }
    (( value >= 50 && value <= 100 )) || { echo 'threshold must be between 50 and 100' >&2; return 2; }

    # Every pack that has the attribute, not just the first: capping one
    # battery of a two-battery machine leaves the other charging to full,
    # which is the opposite of what the person asked for.
    local files=() dir
    while IFS= read -r dir; do
        [[ -e "$dir/charge_control_end_threshold" ]] && files+=("$dir/charge_control_end_threshold")
    done < <(all_battery_dirs)
    (( ${#files[@]} > 0 )) || { echo 'this machine cannot set a charge threshold' >&2; return 1; }

    # tee rather than a redirect: the redirect is performed by the calling
    # shell, which is not the one holding root. One authorization writes every
    # pack.
    "$PANAMA_PATH/bin/panama-sudo" \
        --reason "Capping battery charging at ${value}% to reduce wear" \
        -- sh -c "printf '%s\n' '$value' | tee ${files[*]} >/dev/null" || return 1

    # Read it back rather than reporting success from the write's exit code:
    # some firmware silently clamps or ignores the value.
    read_int "${files[0]}"
}

case "${1:-status}" in
    paths)          cmd_paths ;;
    status)         cmd_status ;;
    set-threshold)  shift; cmd_set_threshold "$@" ;;
    -h|--help)
        cat <<'USAGE'
usage: panama-battery [paths|status|set-threshold <50-100>]

  paths           JSON: which sysfs files hold the battery, mains and threshold
  status          JSON: one reading of charge, state, power source and limit
  set-threshold   cap charging at N percent (asks for a password)
USAGE
        ;;
    *) echo "panama-battery: unknown command: $1" >&2; exit 2 ;;
esac
